Virtual MIDI keyboard
---------------------

Open the "Keyboard" folder and doubleclick the "v.m.k. 1.6 win.exe" to start
the keyboard. If not already installed, a utility program has to be installed
first:

This program is called "LoopBe", and connects the Groven software to the
keyboard inside the computer. (If you already have an internal MIDI bus,
this step is not necessary).


Installation of "LoopBe"
------------------------
Doubleclick the "setuploopbe.exe", and follow the instructions from the setup
program. After installation, an internal MIDI bus will be available.



Using the keyboard with Groven+Sampler
--------------------------------------

- Select "LoopBe" as MIDI port in both programs. In "v.m.k.1.6", click the
   grey field to the right of "Midi Port", and choose "LoopBe Internal MIDI"
   in the popup menu. In Groven+Sampler, select "Audio/MIDI-setup" (green
   button).

- As long as the "v.m.k.1.6" window is selected, it's possible to
   use the mouse or computer keyboard to play the Groven sampler.

- Note that after adjusting settings in the Groven window, the "v.m.k.1.6" window
   has to be selected again to use the computer keyboard, otherwise the
   keys will control the Groven program.
